Primary side of step-up:

* 96V peak-to-peak from h-bridge
* 48V peak

Secondary side of the step-up

* 48V\*3 = 144V Peak
* 288V peak-to-peak
* 101.8233765V RMS