* The current sensor doesn’t need inversion in code because we are grounding the high side of the sense resistor. Negative(into sensor)>Positive(out of inverting opamp)
* The voltage sensor does need inversion in the code